;First lab program : LED’s ON

;-----------------------------------------------------------------------------------------------------------

.include "m32def.inc"

reset: ;Main program entry point on reset

 ldi R16, 0b11111111 ;PA0,1,2,3,4,5,6,7 outputs (STK500 LEDs)

 out DDRB, R16

forever:

 ldi R17, 0b00000000 ;set STK500 LEDs ON

 out PORTB, R17

 rjmp forever ;repeat forever